
*Heaven’s Light is Our Guide*



**DEPARTMENT OF COMPUTER SCIENCE & ENGINEERING**

**Rajshahi University of Engineering & Technology, Bangladesh**

**Surface Crack Detection Using Deep Convolutional Neural Network**

**Author**

Sadman Sakib Radh

Roll No. 1503007

Department of Computer Science & Engineering

Rajshahi University of Engineering & Technology

**Supervised by**

Prof . Dr. Md. Al Mamun

Professor

Department of Computer Science & Engineering

Rajshahi University of Engineering & Technology

**ACKNOWLEDGEMENT**

At first, I would like to thank the Almighty Allah for giving us the opportunity and enthusiasm along the way for the completion of our thesis work.

We would like to express our sincere appreciation, gratitude, and respect to our supervisor Prof. Dr. Md. Al Mamun, Professor of Department of Computer Science and Engineering, Rajshahi University of Engineering and Technology, Rajshahi. Throughout the year he has not only given us technical guidelines, advice and necessary documents to complete the work he has also given us continuous encouragement, advice, help and sympathetic co-operation whenever he deemed necessary. His continuous support was the most successful tool that helped us to achieve our result. Whenever we were stuck in any complex problems or situation he was there for us at any time of the day. Without his sincere care, this work has not been materialized in the final form that it is now at the present.


I am also grateful to all the respective teachers of Computer Science and Engineering, Rajshahi University of Engineering and Technology, Rajshahi for good & valuable suggestions and inspirations from time to time.

Finally, I convey my thanks to my parents, friends, and well-wishers for their constant inspirations and many helpful aids throughout this work.

December 6, 2020                  Sadman Sakib Radh

RUET,Rajshahi

*Heaven’s Light is Our Guide*



**DEPARTMENT OF COMPUTER SCIENCE & ENGINEERING**

Rajshahi University of Engineering & Technology, Bangladesh

***CERTIFICATE***

*This is to certify that this thesis report entitled* ***“Surface Crack Detection using Deep Convolutional Neural Network”*** *submitted by* ***Sadman Sakib Radh, Roll: 1503007*** *in partial fulfillment of the requirement for the award of the degree of Bachelor of Science in Computer Science & Engineering of Rajshahi University of Engineering & Technology, Bangladesh is a record of the candidate own work carried out by him under my supervision. This thesis has not been submitted for the award of any other degree*

Supervisor External Examine

----------------------------------------------- -----------------------------------------------

**Prof. Dr. Md. Al Mamun**

Professor

Department of Computer Science &Engineering

Rajshahi University of Engineering &Technology

Rajshahi-6204

**ABSTRACT**

Crack detection has a major importance for justifying structural health of buildings and roads. As Bangladesh is a densely populated country with a large number of traffic, it is very important to monitor the roads correctly and reduce the chance of accidents and other uncertainty both in roads and buildings. But the task is challenging for computer vision method as cracks have only low-level features for detection which are easily confused with background texture and irregularities in construction. Also the manual process of crack detection is infeasible and time consuming. And the result may not also be accurate all the time. That’s why we are proposing a Machine Learning based algorithm, Deep Convolutional Neural Networks(CNN) for detecting cracks of roads as well as buildings as Convolutional Neural Network is a promising method with higher accuracy and precision. Quantitative evaluation conducted on a data set of 40000 images of size 227 × 227 pixels, are classified in two classes based on the crack and non-crack images. The images are reshaped, rescaled to feed the algorithm while necessary. Throughout the paper we will discuss about the comparative study of CNN for detecting cracks.

*Key words:* Crack Detection, Image processing, Deep Convolutional Neural Network

**CONTENTS**

Page No.

**ACKNOWLEDGEMENT** i

**CERTIFICATE** ii

**ABSTRACT** iii

**CHAPTER 1**

**Introduction** 1-5

1.1 Introduction 1

1.2 Motivation 2

1.3 Literature Review 2

1.4 Thesis Contribution 4

1.5 Thesis Organization 5

**CHAPTER 2**

**Background Study** 6-14

2.1 Computer Vision 6

2.2 Object Recognition 7

2.2.1 An Example 8

2.2.2 Challenges 8

2.2.3 The Image Classification Pipeline 10

2.3 Linear Classifier 11

2.3.1 Score Function 11

2.3.2 Loss Function: Softmax Function 12

2.3.3 One Hot Encoding 13

2.4 Conclusion 14

**CHAPTER 3**

**Neural Networks (NN)** 15-26

3.1 NN 15

3.2 Biological Motivation and Connections 15

3.3 Neural Network Architectures 17

3.4 Data Preprocessing 18

3.5 Weight Initialization 19

3.6 Regularization 19

3.7 Loss Function 21

3.8 Learning 22

3.8.1 Backpropagation 22

3.8.2 Gradient Checks 24

3.8.3 Learning Rate 25

3.8.4 Per-Parameter Adaptive Learning Rate Methods 25

3.9 Conclusion 26

**CHAPTER 4**

**Convolutional Neural Networks (CNN)** 27-39

4.1 CNN 27

4.2 CNN Architecture 28

4.3 Layers in CNN 29

4.3.1 Convolutional Layer 30

4.3.2 Activation Layer 33

4.3.3 Pooling Layer 35

4.3.4 Fully-Connected (FC) Layer 37

4.4 Known Architectures in CNN 38

4.5 Conclusion 39

**CHAPTER 5**

**Methodology** 40-48

5.1 Data Source 40

5.2 Data Preprocessing 42

5.2.2 Image Resize 43

5.2.3 Normalization 43

5.3 Model Architecture 43

5.3.1 Features of VGG16 44

5.3.2 Implementation of The Architecture 45

5.3.3 Training The Model 45

5.4 Conclusion 48

**CHAPTER 6**

**Results and Performance Analysis** 49-52

6.1 Environment 49

6.2 Experimental Analysis 49

6.3 Conclusion 52

**CHAPTER 7**

**Conclusion and Future Works** 53-54

7.1 Summary 53

7.2 Limitations 53

7.3 Future Work 53

7.4 Conclusion 54

**REFERENCES** 55-60

**LIST OF TABLES**

**Table Number** **Table Title** **Page No.**

5.1 Model Summary 47

6.1 Performance of Different Methods 48

**LIST OF FIGURES**

**Figure Number Figure Caption Page No.**

2.1 Computer Vision Tasks 7

2.2 Object Recognition of Different Class 7

2.3 An Example of Object Recognition 8

2.4 Challenges in Object Recognition 9

2.5 CIFAR 10 Dataset 10

2.6 An Example of a Linear Classifier to Failing 12

Predict Correct Class

2.7 Linear Classifier for High Dimensional Points 12

2.8 A One Hot Encoding Example 14

3.1 A Biological Neuron (top) and a Common 16

Mathematical model (bottom)

3.2 An example of a 3-layer neural network 17

3.3 Preprocessing The Data 18

3.4 Dropout Used in a Network 21

3.5 The Change to a Hidden to Output Weight 22

Depends on error

3.6 Loss Function is Changing with Different Learning 25

Rates

4.1 Comparison of an Original Neural Network with a 29

CNN

4.2 A Typical CNN Architecture 30

4.3 ConvNet Architecture Example 30

4.4 Convolution layer example 31

4.5 Example of local connectivity 32

4.6 Activation function: tanh 35

4.7 Activation function: ReLU 35

4.8 Example of maxpooling 36

5.1 Crack images 41

5.2 Non Crack Images 42

5.3 VGG16 Architecture 42

6.1 Accuracy Curve for training and validation 50

6.2 Accuracy Curve for training and validation loss 50

**CHAPTER 1**

**Introduction**

This chapter begins with the motivation behind this thesis topic. Then the literature reviews are discussed right after. Then in the proposed methodology section, the proposed system is described briefly which will solve the problem that is being dealt with. Then, in thesis contribution, contributions of the thesis are outlined. Finally, the chapter ends with a conclusion.

* 1. **Introduction**

Crack detection refers to the process of detecting defects in impermeable materials or surfaces like metals, concrete, ceramics etc. It is very crucial in the inspection and maintenance of concrete as well as roads structures. Traditional approach for crack detection is visual inspection by a trained inspector who evaluates the condition of any surface according to the location and width of a crack. This manual process is very time consuming and is also unfeasible since a building or road may have many cracks at a certain time. And the detection result may not also be accurate all the time.

The image-based crack detection system is thoroughly analyzed in view of the human vulnerability of the inspection. Image analysis approaches classify image cracks on the basis of some hypotheses that cracks are slender and associated regions and darker than their backgrounds [1]. Cracks are typically segmented using the proper threshold [2]. General global transformations and local edge detections are used for more robustness of crack detection, [3-5] such as fast Haar transform, fast Fourier transform, Sobel and Canny edge detectors, etc. Fortunately, this method relies heavily on well-chosen techniques for image preprocessing and image edge detection. And the elements on the surface of the structure are complex and influenced by several real-life influences, such as light, shadows, etc.

Machine learning-based techniques are used to more reliably distinguish cracks from photos [6]. The supervised deep learning algorithms of artificial neural networks

was used to distinguish images with or without cracks [7]. In reality, however, only basic architectures of artificial neural networks can be used to detect cracks due to the constraint of computational capacity. In recent years, In imaging identification, deep CNNs is highlighted [9], thanks to the advancement of deep learning and parallel computations using graphic processing units (GPUs) [8].

In comparison to traditional neural networks, due to the partial ties, exchanging weights and pooling mechanism between neurons, CNNs classifying images rely on less computations. Notably, the CNN infrastructure needs to be developed, and a database containing a large number of images should be built to train CNN[10]. With the prevalence of smartphones, smartphones have been used as instruments for tracking the health of structures[11].

In this paper, a deep CNN network is applied as a classifier for detecting surface crack. The CNN based crack detection can verify cracks from images and the detection result will not be affected by noise on surface or road images.

* 1. **Motivation**

Technological development is going on day by day. The old one is being replaced by the new one. Machine learning based technology is now getting higher popularity. Effective use of such technology is seen in many areas like medical, face recognition etc. As it is a vital issue for safe driving in highways, it is important to ensure the roads are safe. So we need more accuracy with less computational time. And this is only possible through machine based approach like CNN or other models. Some works have been done in this sector and those works have motivated us to develop a classification system that can classify surface crack.

**1.3 Literature Review**

The section is about reviewing some existing works that are related to crack detection. There have been various studies on the road-traffic conditions, causes and their effects in the socio-economic, physical and mental health the people of Bangladesh [12][13][14]. For pattern recognition, image processing, object identification, semantic and instance segmentation, CNN based machine learning models are very efficiently used. So far, the “AlexNet” architecture introduced by Krizhevsky Et al. [15] has been successfully applied in a number of computer vision tasks, for example in object detection [6], object tracking [16], segmentation, [17] video classification, [18] human pose estimation [19] and super resolution [20]. Classical deep Neural Networks like CNN and FCN extract image features finding key points and thus are used for 2D image classification. On the other hand, Google Introduced their own residual deep neural network architecture in Inception-v1, they have optimized the network furthermore through Inception-v3 to reduce computational cost [19][20]. The basic difference between Inception-v3 and Inception-v4 is that the latter one has a simpler architecture and more inception modules [21]. The constraints contained in Inception-v3 had come from the need for partitioning model architecture with distributed training using DistBelief [22]. With migration to TensorFlow [23] those constraints have been lifted which allowed the reintroduced architecture to get simplified.

The goal of this research is to classify crack of any surface or road by using deep convolutional neural network and maximizing the accuracy. 40,000 of crack and non crack images are used for this network. Among them 20,000 are positive (crack) and rest 20,000 are negative (non crack). CNN has been used successfully in 2D

image recognition and research centered on image processing such as: Food Classification [24] and Gaussian noise detection [25]. For this reason, CNN is used to classify crack images. In this analysis, the qualid model evaluated the pixel strength adjustment for the presence of holes, dumps, surfieface water and change in road color for hilly tracts and change in soil.

CNN based researches have been performed to detect road, semantic segmentation of road scenes [26-30], road-lane, road area extraction [31], rural roads detection [32], street signs detection and so on. The works are most commonly based on classification, object detection or semantic segmentation. For image recognition and object-detection based works some of the novel approaches have been introduced by Lin et al. [33], Simonyan et al. in VGGNet [34] and GoogleNet (Inception - v1) [35] by Szededy Et al. Residual connections were introduced in [14]. In civil engineering ventures, deep convolutionary neural network approaches such as bounding box approaches in computer vision-based models have been suggested for surface health monitoring. A model of pothole identification was also proposed[36] based on semantic segmentation on concrete crack images, which is also a fully connected network (FCN) solution. Several semantic image segmentation models have been introduced there by [37-41].

**1.4 Thesis Contribution**

1. An automated system is created using pre-trained Convolutional Neural Network (CNN).
2. The system has the ability to distinguish between crack and non-crack images if it is trained with a large enough dataset.
3. In the training process, it learns the features of different types of crack and then classifies with the learned knowledge.
4. This model can be used in civil engineering sectors.
5. The model leaves opportunities for further improvement and it can be modified for even better results in the future.

**1.5 Thesis Organization**

The rest of the thesis is organized as follows:

**Chapter 2 - Background Study**

This section describes what computer vision and object recognition are and what the challenges and overall computer vision pipeline are. It also describes linear classifier.

**Chapter 3 - Neural Networks**

This chapter discusses the architecture, data preprocessing, weights initialization, loss function, regularization and how learning is achieved in neural networks.

**Chapter 4 - Convolutional Neural Network**

This chapter discusses the architecture, layers and some known popular convolutional neural network models available right now. It also distinguishes the differences between an ordinary neural network and a convolutional neural network.

**Chapter 5 - Methodology**

This chapter describes about the datasets, data preprocessing, the whole work flow of the developed architecture.

**Chapter 6 - Result and Performance Analysis**

This chapter describes the datasets that are used and the overall result of the developed architecture. It also shows the performance of the architecture.

**Chapter 7 - Conclusion and Future Work**

This chapter concludes the thesis, describes its limitation and shows a direction of future work.

**1.6 Conclusion**

Detecting crack is a vital issue in civil engineering. As we are a densely populated country with a large number of vehicles we need to keep the roads safe. The thesis introduces an automated system which can solve this problem.

**CHAPTER 2**

**Background Study**

This chapter starts by describing briefly what computer vision is and then later gives an introduction, method and challenges of object recognition. In the latter part of the chapter, the linear classifier for recognizing objects have been discussed. As the research is based on recognizing crack in surfaces this part is pretty significant to the research work.

**2.1 Computer Vision**

Computer vision is an interdisciplinary area that deals with how machines can be made to interpret visual images or videos at a high level. . High level understanding includes recognizing what the object is (e.g. dog, cat, car etc.), semantic segmentation, classifying using localization to detect a single object in a given scene, instant segmentation and many other tasks depicted in figure 2.1 The idea behind artificial systems that derive information from images is concerned with computer vision. It tries to automate tasks that an animal visual system can do. The target behind computer vision is to create such a system that would be as efficient in recognizing objects and do further actions depending on what kind of object as the human brain sees and does. Almost 50% neurons of a human’s cortex are involved in visual processing [42]. Computer vision aims to mimic the working principles of visual processing in computer processors.

.




Figure 2.1: Computer Vision Tasks [42]

**2.1 Object Recognition**

Object recognition is the process of assigning one mark from a fixed set of categories to an input image. It creates a model that most accurately classifies objects in the given images of the dataset. This is one of Computer Vision's main concerns, which, through its simplicity, has a wide range of practical applications. Figure 2.2 depicts the recognition of different objects.

****

Figure 2.2: Object recognition of different class objects [42]

**2.2.1 An Example**

An object recognition model takes a single image and assigns probabilities to four labels in the image in Figure 2.3, {cat, dog, hat, mug}. An picture is represented as one huge 3-dimensional sequence of numbers as seen in the image. The cat picture in this example is 248 pixels tall, 400 pixels high, and has three red, green, blue, and three color channels (or RGB). The picture, therefore, consists of 248 x 400 x 3 numbers, or 297,600 numbers in total. Each number is an integer ranging between 0 (black) and 2555. (white). The challenge would be to convert this quarter of a million numbers, such as "cat," into a single name.

The task in object recognition is to predict a single label (or a distribution over labels as shown here to indicate our confidence) for a given image. Images are 3-dimensional arrays of integers from 0 to 255, of size Width x Height x 3. The 3 represents the three-color channels Red, Green, Blue.




Figure 2.3: An example of object recognition [42]

**2.2.2 Challenges**

Since this task of recognizing a visual concept (e.g. cat) is relatively trivial for a human to perform, it is worth considering the challenges involved from the perspective of a Computer Vision algorithm. A list of challenges for the computer in the raw representation of images as a 3-D array of brightness values:

* **Viewpoint variation**. With regard to the camera, a single instance of an object may be directed in several ways.
* **Scale variation**. Visual classes often differ in their scale (size in the real world, not only in terms of their extent in the image).
* **Deformation**. Many objects of interest are not static bodies and in extreme cases may be deformed.
* **Occlusion**. It is possible to occlude objects of interest. Often it is only possible to see a small portion of an object (as little as a few pixels).
* **Illumination conditions**. The consequences of illumination on the pixel level are dramatic.
* **Background clutter**. The objects of interest can blend into their surroundings, making it difficult to identify them.
* **Intra-class variation**. The interest categories, such as the chair, may often be relatively large. These objects have several distinct forms, each with its own appearance.

All of these variations must be symmetric to the cross product of a good image classiﬁer, while maintaining sensitivity to the inter-class variations at the same time. Figure 2.4 shows the different challenges for a specific class.




Figure 2.4: Challenges in object recognition [42]

The task is to write an algorithm that can categorize images into different groups. The approach is to provide the program with several samples of each class, instead of attempting to determine what each of the categories of interest looks like explicitly in code, and then create learning algorithms that look at these examples and learn about each class's visual presence. As it focuses on the first aggregation of a training dataset

of labelled images, this approach is referred to as a data-driven approach. The CIFAR10 dataset consisting of 10 groups of 50,000 training images and 10,000 testing images seen in Figure 2.5 will be an instance of this kind.




Figure 2.5: CIFAR 10 dataset

**2.2.3 The Image Classification Pipeline**

In object recognition, the goal is to take a pixel array that represents a single image and give it a name. It is possible to formalize the entire pipeline as follows:

* **Input:** The input consists of a series of N images, each of which is labelled by one of the K groups. This material is known as the training package.
* **Learning:** The learning uses the training package to learn what each class looks like. This phase is known as the teaching of a classifier or the learning of a model.
* **Evaluation:** At the last point, by telling it to predict labels for a new series of images that it has never seen before, the output of the classifier is evaluated. Then it will be compared to the ones projected by the classifier with the true labels of these pictures.

**2.3 Linear Classifier**

An approach to the identification of artifacts that can gradually be applied automatically to whole neural networks and convolutionary neural networks. There will be two key components of the approach: a score function mapping the raw data to class scores, and a failure function quantifying the agreement between the expected scores and the labels of ground truth.

**2.3.1 Score Function**

A training dataset of images , each associated with a label . Here  and .Total of  examples (each with a dimension of ) and  distinct categories. Then a linear mapping can be defined as:

(1)

In the above equation, the image has all of its pixels flattened out to a single column vector of shape [ x 1]. The matrix (of size [ x ]), and the vector (of size [K x 1]) are the parameters of the function. The parameters in are weights, and since influences the output scores is called the bias vector, but without interacting with the actual data . The weights are essential in order to classify the object. In Figure 2.6 explains a linear classifier for an image only having 4 pixels and having only 3 classes (red (cat), green (dog), blue (ship) class). In this classifier, dog score has the highest, meaning it is classifying a cat as dog because of the weights which need to be changed to get the actual results. The next section, it is shown how a loss function changes these weights to get a better result.




Figure 2.6: An example of a linear classifier to failing to predict correct class [42]

And figure 2.7 depicts the analogy of images as high-dimensional points.




Figure 2.7: Linear classifier for high dimensional points [42]

**2.3.2 Loss Function: Softmax Function**

A feature from pixel values to class scores in the previous segment, which was parameterized by a set of weights . As the data cannot be changed, the weights are changed to minimize the loss of the predicted class with the actual class. As seen in the previous section how the classifier failed to predict the correct class. The loss function will determine this outcome to predict the amount of loss in a particular prediction. The loss function softmax is discussed here as it is used the research.

On both names, the Softmax classifier computes "probabilities." For instance, the softmax classifier, given an image, calculates the probabilities of the three labels as [0.9, 0.09, 0.01] for the classes “cat”, “dog” and “ship” which interpret its confidence in each class. For each class, we view the scores in the softmax classifier as the non-normalized log probabilities and quantify loss with a cross-entropy loss that has the form:

(2)

The notation to means the th element of the vector of class scores . The full loss for the dataset is the mean of overall training examples together. The function is called the softmax function: It takes a vector of real-value random scores (in z) and stalks it to a value vector within zero and one that sum to one. The cross-entropy between a “true” distribution and an “estimated” distribution is defined as:

(3)

The Softmax classifier is hence minimizing the cross-entropy between the estimated class probabilities (as seen above) and the “true” distribution, which in this interpretation is the distribution where all probability mass is on the correct class (i.e. contains a single 1 at the position.).

**2.3.2 One Hot Encoding**

Many algorithms for machine learning can not deal directly on label knowledge. They include the numericity of both input variables and output variables. In general, this is often a restriction on the implementations themselves of the effective execution of machine learning algorithms rather than hard constraints. That implies that it is important to transform categorical data into a numerical form. If the categorical variable is an output variable, in order to present it or use it in any application, we may also want to transform model predictions back into a categorical type.

One hot encoding[43] is a method by which categorical variables are translated into a form that could be provided to machine learning algorithms in order to achieve better prediction results. In order to perform "binarization" of the type, we use one hot encoder and include it as a function for model training. The first condition is for integer values to be converted to categorical values. Each integer value is then represented as a binary variable, all of which are zero values, with the exception of the integer index marked with 1.

New (binary) columns are generated by one hot encoding, showing the inclusion of each potential value from the original data. Figure 2.8 gives an example of one hot encoding, with the values in the original data being Red, Yellow, and Green. For each potential attribute, we construct a distinct column. We put a 1 in the Red

column anywhere the initial value was Red.



Figure 2.8: A one hot encoding example [44]

**2.4 Conclusion**

Object recognition is a part of a greater field i.e. computer vision which the process of imitating the vision system of humans. A good classifier is needed for the computer to classify objects with the minimum of loss from the actual results. While working with categorical data, we need a way to turn this into a numerical value.

**CHAPTER 3**

**Neural Networks (NN)**

This chapter discusses different sections of the neural network. Neural network’s motivation and its architecture are briefly explained here. The latter part discusses how the model gets to build and how it is learned through the process.

**3.1 NN**

Also for the human visual system, image recognition based on any basic visual details has always been a hard challenge. Owing to their complicated geometric form as well as the inter-intraclass heterogeneity in the images,they are much more difficult to identify because of the microscopic images from histopathological sections[44]. A deep learning architecture is a trainable neural network. This was promoted by the animal optical system[45] that explicitly learns features from the input data presented, eliminating the hand-crafted function. In several steps, it consists of several nonlinear transformations and works reducing the error to be correctly classified in each step.

**3.2 Biological Motivation and Connections**

To develop an artificial intelligence, through using the combination of basic computational components that approximate the operating process of a human brain, researchers developed a highly integrated device. Researchers originally sought to mimic the neurophysiology of the bran[45] and these components acted as the neurons of the bran. As modern neural networks are now combined with numerous methods of numerical analysis, they will make predictions about various real-world problems[45]. A neuron is the fundamental computational unit of the brain. In the human nervous system, about 86 billion neurons can be identified and are connected to approximately 10^14 - 10^15 synapses[45]. Figure 3.1 shows a drawing of a biological neuron (top) and a common mathematical model (bottom).

Each neuron receives input signals out of its dendrites and produces output signals along its (single) axon. The axon ultimately branches out and connects by synapses to the dendrites of other neurons. The impulses that pass down the axons (e.g. x0) communicate multiplicatively (e.g. w0x0) with the dendrites of the other neuron in the statistical model of a neuron, depending on the synaptic intensity at that synapse (e.g. w0).

The theory is that the synaptic strengths (weights w) are learnable and that the force of one neuron's effect on another is regulated. The dendrites take the signal to the cell body in the fundamental model, where they are all rounded up. The neuron may fire if the final amount is above a certain level, sending a spike down its axon. We believe in the theoretical model that the accurate timings of the spikes do not matter and that information is only transmitted by the frequency of the firing. We model the firing rate of the neuron with an activation function f, which describes the frequency of the spikes along the axon, on the basis of this rate code understanding. Historically, the sigmoid function σ is a typical activation function preference, since it takes a real-valued input (the signal intensity after the sum) and squashes it to a range between 0 and 1. Thus, with the input and its weights, each neuron performs a dot product, adds the bias and applies the non-linearity (or activation function).





Figure 3.1: A biological neuron (top) and a common mathematical model (bottom) [42]

**3.3 Neural Network Architectures**

In an acyclic graph, neural networks are designed as neuron storing that are connected. In other words, certain neurons' outputs can become inputs to other neurons or nodes. Cycles are not permitted and an infinite loop in a network's forward pass would mean that. Versions of the Neural Network are also structured into individual layers of neurons instead of an amorphous blob of connected neurons. The most common layer type for standard neural networks is the fully-connected layer in which nodes are fully pairwise connected between two adjacent layers, but neurons share no connections within a single layer. Figure 3.2 shows a 3-layer neural network with three inputs, two hidden layers of 4 neurons each and one output layer. In both cases there are connections (synapses) between neurons across layers, but not within a layer.



Figure 3.2: An example of a 3-layer neural network [42]

**3.4 Data Preprocessing**

In neural networks, some computer preprocessing methods are used to turn raw data into a comprehensible format. The most popular method of preprocessing is Mean Subtraction. It requires subtracting the mean across each of the data's individual features and has the geometric interpretation of concentrating the data cloud in any axis from the origin.

Normalization refers to the normalization of the proportions of the data such that they are exactly the same height. There are two different methods of doing this normalization. . One is to divide each dimension until it has been zero-centered, by its standard deviation. Each dimension is normalized by another method of this preprocessing, such that the min and max along the dimension are -1 and 1 respectively.It is only used when there are different scales (or units) of different input features, but they should be of about similar significance to the algorithm for learning.

It is only used when there are different scales (or units) of different input features, but they should be of about equal importance to the learning algorithm. Figure 3.3 shows this process in three steps. the red lines in the figure imply the scale of the data - in the centre, they are of unequal length, while on the right they are of equal length.




Figure 3.3: Preprocessing the data [42]

**3.5 Weight Initialization**

The convention is to initialise its parameters before training the network. Setting all initial weights to zero, which is the assumption of "best guess" in expectation, may be a reasonable-sounding idea. But if every neuron or nodes in the network calculates the similar output, then during backpropagation they will also all calculate the same gradients and undergo the exact same parameter updates. In other words, if their weights have been initialized to be the same, there is no cause of asymmetry between neurons. As a solution, initializing the weights of the neurons or nodes to small numbers is usual and refers to doing so as breaking symmetry. The idea is that at the beginning, the neurons are all random and distinct, so they will compute different updates and integrate themselves as diverse components of the entire network. The weight vector of a neuron is initialized with this approximation as a random vector sampled from a Gaussian multi-dimensional, so the neurons point into the input space in the random direction. Since the asymmetry break is given by the small random numbers in the weights, it is possible and normal to initialize the biases to be nil.

The he\_uniform initializer [46] method for weight initialization is an important tool for initializing the weights which are used in this research. The he\_uniform initialization makes surety of the appropriation of the weights, keeping the signal in a fair range of values within many layers. It tries to ensure zero mean and unit variance is the distribution of the inputs to each activation function. It implies that the input data has been normalized to the same distribution in order to do this. In order to compensate for the amount of inputs, the lower the initial weights should be, the greater the number of inputs a neuron has. In a word, the he\_uniform initialization method tries to initialize weights with a smarter value, such that neurons won’t start training in saturation.

**3.6 Regularization**

In order to minimize overfitting, some regularization techniques are implemented in neural networks. L2 regularization is one of them. Perhaps the most common type of regularization is L2 regularization. It can be enforced by explicitly penalizing the square magnitude of all parameters in the target. For each and every weights w in the network, the term is added to the objective, where is the regularization strength. It is usual to see the factor of in front because then the gradient of this term with respect to the parameter is simply instead of . The L2 regularization has an innate knowledge of peak weight vectors being strongly penalized and diffuse weight vectors being favoured.

Another relatively popular method of regularization is L1 regularization, where each weight we have to add the term to the objective. Combining the L1 regularization with the L2 regularization is possible: (this is called Elastic net regularization [47]). The L1 regularization has the interesting property that, during optimization, the weight vectors are becoming sparse (i.e. very close to exactly zero). In other words, L1 regularization neurons end up using just a sparse subset of their most relevant inputs and become almost invariant to the "noisy" inputs. Furthermore, from L2 regularization, there are usually diffuse, small numbers of final weight vectors.

Another method of regularization is to impose an absolute upper limit for each neuron on the magnitude of the weight vector and use the predicted gradient descent to enforce the limitation. This is known as the restrictions of max norm.

Dropout is an extremely effective, simple and recently introduced regularization technique [48]. During preparation, dropout is applied by only having a neuron alive with a certain probability (a hyperparameter), or otherwise setting it to zero. During preparation, it is only feasible to view Dropout as sampling a Neural Network within the complete Neural Network and to change the sampled network parameters depending on the input data. (The exponential number of potential networks sampled, however, is not independent since the parameters are shared.) There is no dropout implemented during research, with the interpretation of measuring an average estimate across all sub-networks' exponentially-sized ensemble. Figure 3.4 illustrates the dropout idea where cross means that the neurons are set to zero (randomly).




Figure 3.4: Dropout used in a network

**3.7 Loss Function**

The lack of data, which phenomenon of supervised learning, tests the consistency between a forecast and the ground truth label (e.g. the class scores in classification). For any particular case, data loss takes the form of an average loss of knowledge. That is, where N is the number of training data and .

If the correct output is a binary vector where every case may or may not have a certain attribute. In this case, the way is to make a binary classifier for every single attribute independently. For example, a binary classifier for each category individually would take the form:

) (4)

where the sum is over all categories , and is either +1 or -1 depending on whether the th example is classified with the th attribute, and the score vector will be positive when the class is predicted to be present and negative otherwise. Remember that if a positive example has a score less than +1, or when a negative example has a score higher than -1, the loss is accrued.

**3.8 Learning**

How the neural network learns through iteration and updates its weights to minimize the loss function will now be discussed.

**3.8.1 Backpropagation**

When training the network there are mostly two passes which need to be completed one after another. The forward pass measures values from inputs to the output, and the backward pass then implies backpropagation that begins at the end and implies the chain rule recursively to measure the gradients all the way to the circuit inputs. To learn the weight of a multilayer neural network with a fixed architecture, the Backpropagation algorithm is used. It tries to minimize the sum square error between the output values of the network and the target values given. For this it performs gradient descent.

Figure 3.5 explains (depicted as a lined pattern) at the output node and activation (depicted as a solid pattern) at the hidden node. Although the adjustment to the hidden weight input depends on the hidden node error (which in turn depends on the error on all the output nodes) and on the input node activation.




Figure 3.5: The change to a hidden to output weight depends on error [42]

For the purpose of this derivation:

* The subscript denotes the output layer.
* The subscript denotes the hidden layer.
* The subscript denotes the input layer.
* denotes a weight from the hidden to the output layer.
* denotes a weight from the input to the hidden layer.
* denotes an activation value (sigmoid function).
* denotes a target value.
* denotes the net input.

In a network, the total error is given by the following equation:

(5)

To reduce this overall loss, we want to change the weight of the network.

(6)

We will begin at the output layer with a particular weight.

(7)

However, the error is not a function of a weight. We expand this as follows.

(8)

In turn, let's consider each one of these partial derivatives. Note that only one term of the summation will have a non-zero derivative: the one connected with the particular weight we are suggesting.

Derivative of the loss or error with respect to the activation:

(9)

Derivative of the activation with respect to the net input:

(10)

Using the activation function’s equation, we can rewrite the result of the partial derivative as:

(11)

Derivative of the net input with respect to a weight:

(12)

Now substituting these results back into our original equation (8), we have:

(13)

This equation is typically simplified as shown below where the term represents the product of the error with the derivative of the activation function.

(14)

We must now decide the necessary shift in weight for an input to a hidden weight.

This is more complex since it relies on the error that this weighted relation will contribute to on all the nodes.

So, the final form it takes: (15)

**3.8.2 Gradient Checks**

It is as easy as comparing the analytic gradient to the numerical gradient to perform a gradient search. The centered difference formula of the form or the finite difference approximation when examining the numerical gradient looks as follows:

(16)

This allows one to calculate the loss function twice to verify every single gradient dimension (so it's about 2 times more costly), but the estimate of the gradient turns out to be much more accurate. To see this, Taylor expansion of and is used which also verifies that the first formula has an error on order of , while the second formula only has error terms on order of .

For comparing the numerical gradient and analytic gradient , introducing the relative error:

(17)

That takes into account the ratio of the differences to the ratio of the absolute values of the two gradients. In practice:

* relative error > usually means the gradient is probably wrong
* > relative error > should be okay.
* > relative error is usually okay for objectives with kinks (Kinks refer to non-differentiable parts of an objective function). But if there are no kinks (e.g. use of tanh nonlinearities and softmax), then is too high.
* and less should be great.

**3.8.3 Learning Rate**

The rate the weights will be updated is called learning rate for the model. The learning rate needs to be controlled as the effects of different learning rates can produce different results and the goal is to reduce the loss function. This is depicted in figure 3.5 as with low learning rates or adaptation rates the improvements will be linear. They are going to look more exponential, with high learning rates. Higher adaptation rates can decrease the loss more efficiently, but they are left with poorer loss values (green line). This is because the optimization involves so much "energy" and the parameters are chaotically jumping around, unable to settle in a pleasant position in the optimization landscape.



Figure 3.6: Loss function is changing with different learning rates [42]

**3.8.4 Per-Parameter Adaptive Learning Rate Methods**

All previous methods that we have addressed so far have manipulated the learning rate for all parameters globally and similarly. Tuning the learning rates or adaptation rates is an expensive process, so much effort has gone into creating techniques that can change the learning rates adaptively, and even do so per parameter. Other hyperparameter settings can also require many of these techniques, but the point is that they are well-behaved for a wider variety of hyperparameter values than the raw learning rate. In this section, we illustrate some common adaptive methods.

**Adagrad:**

Originally proposed by Duchi et al[49], Adagrad is an adaptive learning rate process. The denominator accumulates the square gradients from each iteration in the Adagrad method starting from the beginning of training. This cumulative amount proceeds to develop during training, essentially reducing the learning rate on each dimension, as each term is positive. The cache variable has a size equal to the size of the gradient in this system, and keeps track of the number of square gradients per parameter. This is then used to normalize, element-wise, the parameter update step. The weights receiving high gradients would lower their efficient learning rate, although weights that obtain limited or infrequent updates can increase their efficient rate of learning. The smoothing term “eps” (usually set in the range from to ) avoids division by zero. A downside of Adagrad is that the monotonic learning rate typically proves too aggressive in the case of deep learning and stops learning too early. .

**Adadelta:**

Adadelta is a more stable Adagrad extension that adapts learning rates instead of accumulating all past gradients[50], based on a moving window of gradient updates. This way, even though many changes have been made, Adadelta goes on learning. Over time, the method adapts dynamically using only first order data and has limited computational overhead beyond vanilla stochastic gradient descent.

This learning rate would become infinitesimally tiny after several iterations. The process does not require a learning rate to be manually tuned and appears to be robust to noisy gradient knowledge, different model architecture choices, different data modalities, and hyperparameter selection.

Adagrad's two major disadvantages which were improved in Adadelta:

1. The consistent decrease in learning rates during training
2. The need for a global learning rate that is manually chosen.

**3.9 Conclusion**

Neural network tries to mimic the construction of the human optical system. It is generally consisted of three layers. At first, some minimal data processing is done and the weights are initialized of the network. Then the network is ready to train and the gradient is calculated so the weights can be changed in such a way that the loss of the network will be minimized.

**CHAPTER 4**

**Convolutional Neural Networks (CNN)**

This chapter discussed in detail about convolutional neural network. It explores the architecture of CNN and how it works to solve a problem.

**4.1 CNN**

Convolutional Neural Networks (CNN) are very close to the previously described ordinary neural networks. Neurons or nodes that have learnable weights and prejudices are often made up of CNN. Each neuron receives some inputs, performs a dot product, and with a non-linearity optionally follows it. A single differentiated score function is represented by the entire network: from the raw image pixels on one end to the class scores on the other. And on the last (fully-connected) layer, they scrape a loss function (e.g. SVM/Softmax) just like a regular neural network. The key difference is that ConvNet architectures specifically presume that the inputs are images, so that such properties can be encoded into the architecture by the model. This then allow the forward function more powerful to enforce the number of parameters in the network and reduce them dramatically.

CNN is an enabling architecture of deep learning. This was promoted by the animal optical system[45] that directly learns features from the input data provided, avoiding the hand-crafted function. CNN consists of several nonlinear transformations in several steps and works to decrease the error to be properly classified in each step. In short, a CNN is composed of several trainable stages composed of a stack of data tops, followed by a supervised classifier. Each stage has a set of arrays called feature vectors that represent the vectors of input and output respectively[45]. To train the network, CNN needs a large number of labeled samples and computational resources. Due to the growth of accessible digital data and powerful computing tools, i.e. the Graphics Processing Unit (GPU)[51], the time needed during network training is substantially reduced than before. This convenience will enable us in our environment to train deeper CNN architectures to achieve a higher outcome.

**4.2 CNN Architecture**

Let us clarify how the CNN network converges before going to the info. It is a structured neural network that needs minimal preprocessing to process visual information, where the first pair of layers interconnect sequentially. Since the output of the existing layer is the input of the next layer, CNN is feed-forwarding in nature. There are learnable parameters such as weights and preferences in the CNN neurons. Through a forward move, the network begins teaching itself. The input volume is converted into an output volume by a list of connected layers. At output layer, the prediction is computed as a probability reflecting class scores. In order to compute the error, the expected output is then compared with the actual result. The computed error in backpropagation produces the gradient that flows in the backward direction. The parameters are tuned in such a direction at each stage that the previously produced error [52][53][54] is attempted to decrease. Until the model converges, this process proceeds in an iterative fashion.

Convolution neural Neural Networks benefit from the fact that the input is images and in a more logical way they limit the architecture. In particular, the layers of a ConvNet have neurons organized in 3 dimensions, unlike a standard Neural Network: distance, height, depth. (Note that the word depth here points to the third dimension of the volume of activation, not the depth of a complete neural network, which may relate to the total number of network layers.) Instead of all neurons in a fully-connected way, the neurons in a layer would only be connected to a small region of the layer before it. A ConvNet is generated by layers. Each layer has a simple API: it converts a 3D volume input to a 3D volume output with some distinguishable feature that may or may not have parameters. Figure 4.1 depicts this ConvNet process. From the figure, (Top) A standard 3-layer Neural Network. (Bottom) As visualized in one of the layers, a ConvNet organises its neurons into three dimensions (width, height, depth). The 3D input volume is converted to a 3D output volume of neuron activations by any layer of a ConvNet. The red input layer retains the image in this case, so its width and height would be the image's dimensions, and the depth would be 3. (Red, Green, Blue channels).





Figure 4.1: Comparison of an original Neural Network with a CNN [42]

**4.3 Layers in CNN**

A simple ConvNet is a series of layers, and through a distinctive feature, each layer of a ConvNet transforms one volume of activations into another. To build ConvNet architectures, three main layer types are required: Convolutional Layer, Pooling Layer, and Fully-Connected Layer (precisely as seen in regular Neural Networks). To form a complete ConvNet architecture, stack these layers together. Figure 4.2 shows a typical CNN architecture.




Figure 4.2: A typical CNN architecture [45]

Figure 4.3 describes the activations of an example ConvNet architecture. The raw image pixels are stored in the initial volume (left), and the last volume stores the class scores (right). As a column, each volume of activations along the processing path is shown. Since visualizing 3D volumes is hard, we spread out the slices of each volume in rows. For each class, the last layer volume contains the scores, but here we only visualize the top 5 scores sorted and print the labels of each one.






Figure 4.3: ConvNet architecture example [42]

**4.3.1 Convolutional Layer**

The Conv layer is a Convolutional Network's main building block that performs much of the heavy computational lifting. The parameters of the CONV layer consist of a series of learnable filters. Each filter is spatially small (along with width and height), but it extends to the maximum depth of the input volume. A standard filter on the first layer of a ConvNet, for example, may have a size of 5x5x3 (i.e. 5 pixels for width and height, and 3 because the images are of depth 3, the color channels). During the forward pass, each filter is slid i.e. convoluted across the width and height of the input volume and calculate dot products among the entries of the filter and the input at any position.

We will generate a 2-dimensional activation map as we slide the filter over the width and height of the input volume, providing the results of that filter at every spatial position shown in Figure 4.4. Intuitively, when they see any kind of visual features, such as an edge of some alignment or a blotch of some color on the first layer, the network will learn filters that enable, or eventually entire honeycomb or wheel-like patterns on higher layers of the network. Now, in each CONV layer, we will have a whole set of filters (e.g. 12 filters), and each of them will generate a different 2-dimensional activation map. These activation maps will be stacked along the depth dimension and the output volume will be generated.



Figure 4.4: Convolution layer example [42]

An example in figure 4.5 shows (Top) an input volume in red (e.g. a 32x32x3 CIFAR-10 image), and an example volume of neurons or nodes in the first Convolutional layer. In the convolutional layer, each neuron is spatially linked only to a local region in the input volume not to the maximum depth (i.e. all color channels). There are many neurons (5 in this example) along its depth, all in the input looking at the same area (Bottom). The neurons from the Neural Network chapter remain unchanged: with the input followed by a non-linearity, they still measure a dot product of their weights, but their connectivity is now limited to being spectrally local.





Figure 4.5: Example of local connectivity [42]

The size of the output volume is regulated by three hyperparameters: width, stride, and zero-padding. A hyperparameter is the depth of the output volume: it corresponds to the number of filters that are being used to each learning to scan for something different in the input. The number of the stride must be specified with which we slide the filter. When the stride is 1, then one pixel at a time, we pass the filters. When the stride is 2 (or uncommonly 3 or more, though this is an uncommon practice) then the filters dive 2 pixels at a time as we slide them around. This will create smaller spatial production volumes. Finally, It is sometimes easy to pad the input volume along the boundary with zeros. The zero-padding scale is a hyperparameter. The nice feature of zero padding is that it will allow us to control the spatial size of the output volumes.

The spatial size of the output volume can be calculated as a function of the input volume size (), the receptive field size of the Conv Layer neurons (), the stride with which they are applied () and the amount of zero padding used () on the border. In general, setting zero padding to be when the stride is guarantees the spatially equivalent scale of the input volume and output volume.

**4.3.2 Activation Layer**

The activation layer presents the network with non-linear features accompanied by convolution layers. Their primary aim is to turn a node's input signal into an output signal. The output generated will be passed on to the next layer. A single number is taken by any activation function (or non-linearity) and conducts a certain fixed mathematical operation on it. There are many activation functions to choose from. Two activation functions are discussed here.

**Sigmoid: The mathematical form of sigmoid is and that is shown in figure 4.6. It requires a real-valued number and “squashes” it into a range between 0 and 1. In particular, large negative numbers become 0 and large positive numbers become 1. The sigmoid function has seen frequent use since it has a nice interpretation as the firing rate of a neuron: from not firing at all (0) to fully-saturated firing at an assumed maximum frequency (1). Sigmoid non-linearity has recently fallen out of favor in practice and is seldom used. It has two big downsides:**

1. A very unfavorable characteristic of the sigmoid neuron is that the gradient at these regions is almost zero when the activation of the neuron saturates at either tail 0 or 1. Therefore, if the local gradient is very small, it will effectively “kill” the gradient and almost no signal will flow through the neuron to its weights and recursively to its data.
2. Sigmoid outputs are not zero-centered. This is undesirable since neurons in later layers of processing in a Neural Network (more on this soon) would be receiving data that is not zero-centered.

**ReLU: In the past few years, the Rectified Linear (ReLU) Unit has become very widely known. It is efficient in computation and converges much rapidly than most other activation functions** [14]. **It computes the function showed in figure 4.7. The activation is simply being the threshold at zero (see image above on the left). The use of the ReLUs has several pros and cons:**

1. The convergence of stochastic gradient descent compared to the sigmoid functions was found to greatly accelerate.
2. The ReLU can be implemented by simply thresholding a matrix of activations at zero roughly equivalent to sigmoid neurons that involve costly operations (exponentials, etc.).
3. Unfortunately, during training, ReLU units can be delicate and can' die.' A large gradient flowing through a ReLU neuron, for example, could cause the weights to be updated in such a way that no data point will ever activate the neuron again. If this happens, then from that point on, the gradient flowing through the unit will permanently be zero. That is, as they can get knocked off the data manifold, the ReLU units can die irretrievably during training.




Fig 4.6: Activation function: tanh



Figure 4.7: Activation function: ReLU

**4.3.3 Pooling Layer**

Periodic insertion of a pooling layer in a ConvNet architecture between successive Conv layers is normal. In order to reduce the number of parameters and computation in the network, its purpose is to gradually reduce the spatial size of the representation, and thus also to regulate overfitting. On each depth slice of the input, the Pooling Layer works independently and resizes it spatially, using the MAX operation. The most familiar example is a pooling layer with 2x2 size filters implemented with a step of 2 downsamples in each slice of depth in the input by 2 along both width and height, dismissing 75% of the activations. In this case, each MAX operation will take a max of 4 numbers (little 2x2 region in some depth slice). The dimension of depth remains unaltered. More typically, the pooling layer:

* Accepts a volume of size
* Requires two hyperparameters:
  + their spatial extent ,
  + the stride  ,
* Produces a volume of size where:
  + +1
* Introduces zero parameters since it calculates a fixed function of the input
* For Pooling layers, it is unfamiliar to pad the input using zero-padding.

The pooling layer spatially downsamples the volume, independently of the input volume in each depth slice. In this example of figure 4.8, (top) the input volume of size [224x224x64] is pooled with filter size 2, stride 2 into output volume of size [112x112x64]. Note that the depth of the volume is retained. (Bottom) The most familiar downsampling operation is max, giving rise to max pooling, here shown with a stride of 2. That is, 4 numbers are taken over by each limit (little 2x2 square).





Figure 4.8: Example of maxpooling [42]

**4.3.4 Fully-Connected (FC) Layer**

As seen in normal Neural Networks, neurons in a completely connected layer have complete connections to all activations in the previous layer. With a matrix multiplication followed by a bias offset, their activations can therefore be computed. It should be remembered that the only distinction between the FC and CONV layers is that the neurons in the CONV layer are only bound at the input to a local region and that all of the neurons share a parameter in the CONV volume. However, dot products are still computed by the neurons in both layers, so their functional form is similar. It is also possible to transform between FC and CONV layers, it turns out.

* There is an FC layer for any CONV layer which applies the same forward function. The weight matrix will be a large matrix that is completely zero, except in some blocks (due to local connectivity) where the weights are identical in many of the blocks (due to parameter sharing).

Contrarily, it is possible to transform every FC layer to a CONV layer. An FC layer with K=4096, for example, that looks at some input volume of size 7 x 7 x 512, can be interpreted equally as a CONV layer with F=7,P=0,S=1,K=4096. In other words, we set the filter size to be exactly the right size of the input volume, so the output is simply 1 x 1 x 4096 since only a single column of depth "fits" throughout the input volume, giving the same result as the original FC layer.

Depending on the number of classes in the classification task, the final fully connected layer of the network generates the net output with an activation function, i.e. softmax, which gives the same result as the initial FC layer. A standard CNN architecture comprises of these types of multiple components. An example of a standard architecture would be:

[(CONV-RELU)\*N-POOL?]\*M-(FC-RELU)\*K,SOFTMAX

where N is usually up to ~5, M is large, 0 <= K <= 2.

**4.4 Known Architectures in CNN**

There are several architectures in the field of Convolutional Networks that have a name. The most common are:

* **LeNet:** Yann LeCun developed the first successful implementations of Convolutional Networks in the 1990s. The best known of these is the LeNet architecture[34], which has been used to read zip codes, digits, etc.
* **AlexNet**: AlexNet[14], developed by Alex Krizhevsky, Ilya Sutskever and Geoff Hinton, was the first work that pioneered Deep convolutional Networks in Computer Vision. The Network had a very similar design to LeNet, but it was stacked on top of each other deeper, wider, and featured Convolutional Layers (previously it was normal to have only a single CONV layer often immediately followed by a POOL layer.
* **GoogLeNet**: The ILSVRC (Large Scale Visual Recognition Challenge) 2014 winner was a CN (Convolutional Network) from Szegedy et al. [47] from Google. The key contribution was the design of an Inception Module that significantly decreases the amount of network parameters (4M, compared to AlexNet with 60M). In contrast, rather than completely connected layers at the top of the ConvNet, this paper uses Average Pooling, excluding a large number of parameters and do not seem to concern much.
* **VGGNet**: The runner-up in ILSVRC 2014 was the network from Karen Simonyan and Andrew Zisserman that became known as the VGGNet [48]. Its major contribution was to demonstrate that a critical component of good performance is the depth of the network. There are 16 CONV/FC layers in their current optimal network and, alluringly, features an extremely homogeneous architecture that only conducts 3x3 convolutions and 2x2 pooling from start to finish.
* **ResNet:** Residual Network constructed by Kaiming He et al. [49] was the winner of ILSVRC 2015. Special skip connections and a heavy use of batch normalization are featured in it. Also, at the end of the network, the architecture lacks fully connected layers. Kaiming's presentation (video, slides), and some recent experiments reproducing these networks in Torch are also referred to by the reader. Presently, ResNets are state-of-the-art Convolution Neural Network models and are the preferred option in procedure for using ConvNets.

**4.5 Conclusion**

CNN is another form of the ordinary neural network but it takes images as inputs. CNN architectures are mainly constructed by some major layers and they are stacked one after another.

**Chapter 5**

**Methodology**

This chapter consists of the work flow throughout the research. It includes data collection, building databank for training and validation set, developing deep CNN for training, classifying crack and non crack images.

**5.1 Data Source**

The datasets are collected [55]. The datasets include pictures of different textures of concrete with and without cracking. The image data is split into two in a separate folder for image classification as negative (without crack) and positive (with crack). With a total number of 40000 images of 227 x 227 pixels with RGB channels, each class has 20000 images. The dataset is created from 458 (4032x3024 pixel) high-resolution images using the method proposed by Zhang et al (2016) [56]. High-resolution photographs have been shown to have high differences in terms of surface finish and state of lighting. For random rotation or flipping or tilting, data augmentation is not implemented.





Fig 5.1: Crack Images[55]

Fig 5.2: Non-Crack Images[55]

All the images are in JPG Format. This a balanced dataset with equally distributed crack and non-crack images.

**5.2 Data Preprocessing**

I have spent a fair amount of time on strategies for data preprocessing typically used for image processing. This is because in most deep learning applications, preprocessing takes a large amount of time. As the dataset contains 40,000 images with RGB channel, I’ve performed two image processing techniques.

**5.2.1 Image Resize**

The first step in data pre-processing is the creation of images of the same size to feed our pre-trained CNN model. For this I’ve used keras built in function[57]. The images are re-sized into 150 x 150.

**5.2.2 Normalization**

Image normalization is a method often used in the preparation of machine learning data sets in which multiple images are positioned in a standard statistical distribution in terms of scale and pixel values; but within themselves, a single image may also be normalized. Typically, the phase entails both spatial and intensity normalization.

This is the most crucial step in image pre-processing. This corresponds to rescaling the values of the pixels so that they lie within a confined range. One of the reasons for doing so is to help with the challenge of gradient propagation. For normalization I’ve divided each pixel by 255 and re-scaled them between 0 to 1.

**5.3 Model Architecture**

For the classification I’ve used pre-trained CNN model VGG16 [58]. VGG is an acronym for the Oxford University Visual Geometric Group, and VGG-16 is a network suggested by the Visual Geometric Group with 16 layers. The trainable parameters are found in these 16 layers and there are other layers, such as the Max pool layer, but there are no trainable parameters. This architecture was the first heir to the 2014 Visual Perception Competition, i.e. ILSVRC-2014 which was founded by Zisserman and Simonyan. Figure 5.3 shows a VGG16 architecture.


****

Fig 5.3: VGG16 Architecture[57]

The model is simple. It has 2 contiguous blocks of 2 convolution layers, followed by max-pooling, then it has 3 contiguous blocks of 3 convolution layers, followed by max-pooling. The convolutional layers are the hidden layers of VGG16. The hidden layers extract the features. 3 fully connected layers follow the stack of the convolutional layers. In different architectures, the last 3 layers of convolution have different depths.

**5.3.1 Features of VGG16 Network**

1. **Input Layer:** It accepts color images with a resolution of 224 x 224 and 3 channels as an input, i.e. Red, Green, and, in reality, Blue.ConvNets.
2. **Convolution Layer:** The images pass through a series of convolution layers with a very limited receptive filter of 3 x 3 and stride 1 for each convolution filter. Each convolution filter uses padding for rows and columns such that the input size and output feature maps remain identical or, in other words, the resolution remains the same after the convolution is implemented.
3. **Max pooling:** It is applied over a 2 x 2 max pool window with phase equal to 2, which means that max pool windows are non-overlapping windows here.
4. Max pool layer does not follow every convolutional layer as there are some consecutive convolutional layer following each other at some places without having a max pool layer between them.
5. The first two fully connected layers are of having 4096 channels each. And the final layer in another fully connected layer which is the output layer actually having 1000 channels, one for each category of images in the imagenet database.
6. ReLU function was used in the convolutional layers or the hidden layers.

**5.3.2 Implementation of The Architecture**

The input to the conv1 layer is a fixed image size of 224 x 224 RGB. The image is passed through a series of convolutional layers (conv.) where the filters have been used with a very narrow receptive field: 3 x 3 (which is the smallest size to catch the left/right, up/down, center). It also uses 1 x 1 convolution filters in one of the setups, which can be used as a linear transformation of the input channels (followed by non-linearity). The convolution stride is fixed to 1; conv's spatial padding. The layer input is such that after convolution, the spatial resolution is retained, i.e. the padding for 3 x 3 conv is 1-pixel. Of textures. Five max-pooling layers, which obey some of the conv, perform spatial pooling. Of textures (not all the conv. layers are followed by max-pooling). Max-pooling, with stride 2, is done over a 2 to 2 pixel window.

A series of convolutional layers (which depth varies in different architectures) is preceded by three Fully-Connected (FC) layers: the first two are of 4096 channels each, the third has 1000-way (which is the output) ILSVRC classification and thus includes 1000 channels (one for each class). The last layer is soft-max layer. The configuration of fully linked layers on all networks is the same.

Both hidden layers are fitted with non-linearity for rectification (ReLU). Furthermore, it is remembered that none of the networks (except for one) contain Local Response Normalization (LRN), which does not boost the efficiency of the ILSVRC dataset, but results in increased memory usage and computation time.

**5.3.3 Training The Model**

As it is mentioned earlier about the proposed CNN model. For training the model the validation set was splitted from entire dataset. A validation dataset is a dataset of examples used for tuning a classifier's hyperparameters. Often it is also referred to as the “Development set” or the "dev set". The number of hidden units in each layer includes an example of a hyperparameter for machine learning.

For proposed method about 30 percent of the total dataset was used for validation. The validation set was selected randomly. So 12000 images were reserved for validation and rest 28000 images were used for training containing both crack and non crack images. After that the training and validation data were feed into VGG16 model. For VGG16 the weights are initialized with “imagenet” [59] a pretrained model weight initialization. The batch size is 64 and epoch is 20. VGG16 has 5 block with 13 convolutional layer. So the training and validation dataset are fast go through 5 blocks of VGG16. After that the output is flattened from 4 x 4 x 512 to 8192 x 1 which is a one dimensional vector. The series of convolutional layers were followed by two fully connected layers. The first one has 1024 channels and final layer is ‘sigmoid’ layer which classifies the image into crack or non crack.

Validation and testing were performed in training period. ‘ReLU’ function was used in each hidden layers. It is effective in computing and converges much faster than most other activation functions. “ReLU” converts the negative calculated value to 0 and no negative value passes to next layer. Hidden layers are the feature extracting layer. So using “ReLU” function in hidden layers doesn’t effect the output much because of the ignorance of the negative values. “Sigmoid” is used in final layer. **The mathematical form of sigmoid non linearity is . It takes a real-valued number and “squashes” it into a range between 0 and 1. In particular, large negative numbers become 0 and large positive numbers become 1. As the input dataset is binary class sigmoid function merges the output into crack or non crack images. 0 for non crack image and 1 for crack image.**

“Dropout” is used before the output layer to overcome the overfitting problem in the network [48]. Overfitting is' the development of a study that correlates too closely or precisely to a specific data set and may therefore struggle to match additional data or accurately predict future findings.' An overfit model is a mathematical model containing more parameters than the data can explain [60]. To overcome this problem dropout is used. Dropout is a system where, during training, randomly selected neurons are dropped. They are arbitrarily "dropped-out." This means that on the forward pass, their contribution to the activation of downstream neurons is temporarily evacuated and any weight refreshments are not added to the backward pass neuron. The dropout was 20 percent in proposed method. It means 20 percent of total nodes were set to zero randomly.

The network is trained all over using Adam optimizer with initial standard parameters [60]. During training the network weights may stack into local minima problem. Adam helps to find the global minima when the network stacks into local minima problem. Adam updates network weights iterative based in training data.

The model has two classes, crack and non crack. Regarding the problem “binary\_crossentropy” function was used to minimize the error [57]. It is very easy to train a model for binary\_crossentropy to solve many classification problems at the same time. , if each classification can be reduced to a binary choice. The crack detection is a binary classification task. The output is a binary label ; representing the absence of crack or not respectively. In the training set, weighted binary cross entropy loss was optimized. A table of the summary of the whole network is given below:

Table 5.1 Model Summary

|  |  |  |
| --- | --- | --- |
| **Layer(Type)** | **Output Shape** | **No of Parameter** |
| **input** | (150, 150, 3) | 0 |
| **block1\_conv1** | (150, 150, 64) | 1792 |
| **block1\_conv2** | (150, 150, 64) | 36928 |
| **block1\_pool** | (75, 75, 64) | 0 |
| **block2\_conv1** | (75, 75, 128) | 73856 |
| **block2\_conv2** | (75, 75, 128) | 147584 |
| **block2\_pool** | (37, 37, 128) | 0 |
| **block3\_conv1** | (37, 37, 256) | 295168 |
| **block3\_conv2** | (37, 37, 256) | 590080 |
| **block3\_conv3** | (37, 37, 256) | 590080 |
| **block3\_pool** | (18, 18, 256) | 0 |
| **block4\_conv1** | (18, 18, 512) | 1180160 |
| **block4\_conv2** | (18, 18, 512) | 2359808 |
| **block4\_conv3** | (18, 18, 512) | 2359808 |
| **block4\_pool** | (9, 9, 512) | 0 |
| **block5\_conv1** | (9, 9, 512) | 2359808 |
| **block5\_conv2** | (9, 9, 512) | 2359808 |
| **block5\_conv3** | (9, 9, 512) | 2359808 |
| **block5\_pool** | (4, 4, 512) | 0 |
| **flatten** | (None, 8192) | 0 |
| **Dense** | (None, 1024) | 8389632 |
| **Dropout** | (None, 1024) | 0 |
| **Dense** | (None, 1) | 1025 |

**5.4 Conclusion**

The chapter is about the methodology of building the architecture. VGG16 is a pretrained architecture with total number of five blocks containing thirteen convolutional layer distributed in each block. Each block has a maxpooling layer following the convolutional layers.

**CHAPTER 6**

**Results and Performance Analysis**

This is the result analysis chapter. Through out the chapter the result of the method will be discussed.

**6.1 Environment**

The VGG16 model was built in kaggle notebook [58]. The notebook editing session allows 9 hours execution time. It has 20 Gigabytes of auto saved disk including 4 CPU cores, 16 Gigabytes of RAM. And the GPU specs with 2 CPU cores and 13 Gigabytes of RAM. It provides NVIDIA Tesla P100. Keras API on top of TensorFlow (CUDA toolkit 9.0, cuDNN SDK v7 and python 3.6) were used [59].

**6.2 Experimental Analysis**

The data set is divided into training and validation set randomly. 12000 images were selected for validation and the rest for training. Testing was performed during training period. The results presented in this work is based on accuracy and f1 score [60] which are defined by the following equations:

(20)

(21) 

Where tp, tn, fp, fn represent respectively true positive, true negative, false positive and false negative. In a dataset that is successfully retrieved, recall is defined as the fraction of the relevant instances and precision reflects the proportion of the data points that the model says are actually relevant.

Instead of manual feature extraction methods, CNN has the benefit of learning features automatically. The CNN model's self-learning capability provides convenience than the typical system of learning.

Figure 6.1 shows the training and validation accuracy and figure 6.2 shows the training and validation loss.




Figure 6.1: Accuracy curve for training and validation




Figure 6.1: Accuracy curve for training and validation loss

From the figure we can see, by the increasing number of epochs the proposed model gets more accuracy with a decreasing factor of loss. It took around 233s for first epoch and gradually the time was minimized. Using equations (20) and (21), the proposed system achieved 99.90 percent accuracy, 0.990 f1 score and 0.9992 precision which outperformed the previous state of the art. A recent research [30] had the accuracy of 97.5 percent accuracy using ResNet based classifier. Though VGG16 got 99.8 percent accuracy but needed 50 epoch to acquire this accuracy which was very time consuming. Proposed method got almost same accuracy performing only 20 epoch which was very much time friendly. Performance of different of CNN architecture is shown in the table below comparing the proposed model also:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Method** | **Accuracy** | **Recall** | **Precision** | **F1 Score** |
| VGG16 | 99.8% | 0.999 | 0.998 | 0.998 |
| Inception V3 | 99.7% | 0.997 | 0.998 | 0.997 |
| ResNet | 97.5% | 0.945 | 0.994 | 0.968 |
| Proposed VGG16 | 99.9% | 0.9988 | 0.9992 | 0.9990 |

Table 6.1: Performance of Different Methods

From the table we can see proposed method has outperformed in all the field including accuracy, precision, recall and f1 score.

The accuracy of the network highly depends on the depth of CNN architecture [62]. VGG16 is a deep convolutional neural network with 13 convolutional layer and three fully connected layer. The hidden layers of CNN extract the features. That’s why VGG16 performs better for feature extracting methods.

“ReLU” is the activation function of VGG16 in hidden layers. It computes the function  **and the activation being threshold at zero. Compared to ‘Sigmoid’ function which has exponential operations ‘ReLU’ can be implemented by simply thresholding a matrix of activation at zero.**

**The kernels are initialized with ‘imagenet’ initializer [58]. This is pretrained weight for VGG16. Three ‘fully connected’ layers were used in the network.** The network was trained with Adam optimizer with initial standard parameters. Adam is an algorithm for optimization that can be used to adjust iterative network weights based on training data instead of the classical stochastic gradient descent technique. Previous methods used ‘RMSProp’, ‘AdaGrad’[30] etc optimization tools. But among them Adam showed the best optimization in proposed method.

**6.3 Conclusion**

The proposed method achieved a quite good accuracy detecting crack images. This methodology can contribute a lot in detecting cracks in civil engineering sectors.

**CHAPTER 7**

**Conclusion and Future Works**

This chapter discusses the summary of thesis work, its limitation and shows future work direction.

**7.1 Summary**

The motivation of this research work is to build a machine learning image classification model that have a decent accuracy to classify the crack on surface or road. It is very important to identify the cracks of a building or road in civil engineering sectors. Manually detecting cracks is very time consuming and may not also accurate all the time. The proposed method can detect the crack with a decent accuracy. A 40,000 images of crack and non crack were taken for the method. Some of the images were noisy, some of them consists of dust, shadows etc. The proposed method can handle those problems. The images were 227x227 pixels of size with RGB channel. It was reduced to 150x150 pixels with RGB channel to feed the network and reduce the computational time and complexity. Six layers of convolution were used attaching maxpooling layer in each. And three fully connected layers were used. Finally the result of the architecture came quite good with decent accuracy. Using optimized hyperparameters to enhance device accuracy, future work will explore various architectures.

**7.2 Limitations**

We worked with only one data source to train our model. With a bigger dataset and more data sources, we would have more variant data samples where the model can be more generalized for detecting cracks. Besides we did not develop any mobile applications for detecting cracks. With the proposed method mobile application can be developed and cracks can be identified.

**7.3 Future Work**

The plan is to keep working with object recognition and explore other domains related to this. The plan includes:

* We want to work with other object recognition challenges and try to achieve the state of art accuracy in the respective domain.
* We also want to develop:
  + A new hybrid model architecture which would work to recognize objects much better.
  + Ensemble between different models to achieve greater results.
  + Extract additional features and fusion with CNN architecture for better accuracy.
  + More optimized Hyperparameters.

**7.4 Conclusion**

In the present study, a pretrained model of CNN is proposed for concrete crack detection. The model performs better than ResNet classifier and gives almost same performance against VGG16 classifier and Inception V3 classifier. The model also needs less time than any other model because of using only 20 epoch. Though the proposed method capture cracks in path, quantifying crack size autonomously is still challenging when an image contains so much noises. Therefore, future studies should focus on how to improve the proposed method more robust to make autonomous crack detection.

**References**

[1] Yamaguchi, T., Nakamura, S., Saegusa, R., and Hashimoto, S., “Image‐based crack detection for real concrete surfaces,” IEEJ T. Electr. Electr. 3(1), 128-135 (2010).

[2] Oliveira, H. and Lobato Correia, P. “Automatic road crack segmentation using entropy and image dynamic thresholding,” Proc. EUSIPCO 2009, 622-626 (2009).

[3] Santhi B., Krishnamurthy G., Siddharth S., Ramakrishnan P.K., “Automatic detection of cracks in pavements using edge detection operator,” J. Theor. App. Inf. Technol. 36(2), 199-205 (2012).

[4] Abdelqader, I., Abudayyeh, O., and Kelly, M. E., “Analysis of edge-detection techniques for crack identification in bridges,” J. Comput. Civil Eng. 17(4), 255-263 (2003).

[5] Yeum, C. M. and Dyke, S. J., “Vision‐based automated crack detection for bridge inspection,” Comput.- Aided Civ. Infrastruct. Eng. 30(10), 759-770 (2015).

[6] Liu, S. W., Huang, J. H., Sung, J. C., and Lee, C. C., “Detection of cracks using neural networks and computational mechanics,” Comput. Methods Appl. Mech. Engrg. 191(25–26), 2831-2845 (2002).

[7] Moselhi, O. and Shehab-Eldeen, T., “Classification of defects in sewer pipes using neural networks,” J.Infrastruct. Syst. 6(3), 97-104 (2000).

[8] Lecun, Y., Bengio, Y., and Hinton, G., “Deep learning,” Nature. 521(7553), 436 (2015).

[9] Krizhevsky, A., Sutskever, I., and Hinton, G. E., “ImageNet classification with deep convolutional neural networks,” International Conference on Neural Information Processing Systems, 60, 1097-1105 (2012).

[10] Deng, J., Dong, W., Socher, R., Li, L. J., Li, K., and Li, F. F., “ImageNet: A large-scale hierarchical image database,” Proc. CVPR 2009, 248-255 (2009).

[11] Zhao, X. F., Han, R. C., Yu, Y., Hu, W. T., Jiao, D., Mao, X. Q., Li, M. C, and Ou, J. P., “Smartphone-based mobile testing technique for quick bridge cable–force measurement,” J. Bridge Eng. 22(4), 06016012 (2016).

[12] A. A. Haider, “Traffic jam: The ugly side of Dhaka's development,” [Online], Available: https://www.thedaily star .net /opinion/society/traffic jam-the-ugly-side-dhakas-development-1575355. [Accessed Dec 14, 2019].

[13] K. Mahmud, K. Gope, S. Mustafizur, and S. Chowdhury, “Possible Causes & Solutions of Traffic Jam and Their Impact on the Economy of Dhaka City” Journal of Management and Sustainability, Volume 2, 2012.

[14] K. He, X. Zhang, S. Ren, and J. Sun, “Deep residual learning for image recognition”, arXiv preprintarXiv:1512.03385, 2015*.*

[15] R. Shamsher, and M. Abdullah, “Traffic Congestion in Bangladesh- Causes and Solutions: A study of Chittagong Metropolitan City,” Asian Business Review, Volume 2, March 2015.

[16] A. Krizhevsky, I. Sutskever, and G. E. Hinton, “Imagenet classification with deep convolutional neural networks”, In Advances in neural information processing systems, pages 1097–1105, 2012

[17] R. Girshick, J. Donahue, T. Darrell, and J. Malik, “Rich feature hierarchies for accurate object detection and semantic segmentation”, In Proceedings of the IEEE Conference on Computer Vision and Pattern Recognition (CVPR), 2014.

[18] N. Wang and D.-Y. Yeung, “Learning a deep compact image representation for visual tracking”, In *Advances in Neural Information Processing Systems,* pages 809–817, 2013*.*

[19] J. Long, E. Shelhamer, and T. Darrell, “Fully convolutional networks for semantic segmentation”, In Proceedings of the IEEE Conference on Computer Vision and Pattern Recognition, pages 3431–3440, 2015.

[20] A. Karpathy, G. Toderici, S. Shetty, T. Leung, R.Sukthankar, and L. Fei-Fei, “Large-scale video classification with convolutional neural networks”, In Computer Vision and Pattern Recognition (CVPR), 2014 IEEE Conference on, pages 1725–1732. IEEE, 2014.

[21] A. Toshev and C. Szegedy, “Deeppose: Human pose estimation via deep neural networks”, In Computer Vision and Pattern Recognition (CVPR), 2014 IEEE Conference on, pages 1653–1660. IEEE, 2014.

[22] C. Dong, C. C. Loy, K. He, and X. Tang, “Learning a deep convolutional network for image super-resolution”, In Computer Vision–ECCV 2014, pages 184–199. Springer, 2014*.*

[23] C. Szegedy, V. Vanhoucke, S. Ioffe, J. Shlens, and Z.Wojna, “Rethinking the inception architecture for computer vision”, arXiv preprint arXiv:1512.00567, 2015.

[22] J. Eriksson, L. Girod, B. Hull, R. Newton, S. Madden, and H. Balakrishnan, “The pothole patrol: using a mobile sensor network for road surface monitoring,” In Proceedings of the 6th international conference on Mobile systems, applications, and services (MobiSys'08), New York, USA, June 17 - 20, pp. 29-39.

[23] M. Abadi, A. Agarwal, P. Barham, E. Brevdo, Z. Chen, C. Citro, G. S. Corrado, A. Davis, J. Dean, M. Devin, S.Ghemawat, I. Goodfellow, A. Harp, G. Irving, M. Isard, Y. Jia, R. Jozefowicz, L. Kaiser, M. Kudlur, J.Levenberg, D. Mane, ´ R. Monga, S. Moore, D. Murray, C. Olah, M. Schuster, J. Shlens, B. Steiner, I. Sutskever, K. Talwar, P. Tucker, V. Vanhoucke, V. Vasudevan, F.Viegas, O. Vinyals, P. War- ´den, M. Wattenberg, M.Wicke, Y. Yu, and X. Zheng. TensorFlow: Large-scale machine learning on heterogeneous systems, 2015. Software available from tensorflow.org.

[24] A. Goswami and H. Liu, "Deep Dish: Deep Learning for Classifying Food Dishes,"(2017) [Online], Available: https://www.semanticscholar.org/paper/Deep-Dish-%3A-DeepLearning-for-Classifying-Food-GoswamiMicrosoft/2e596abd9d4616f75c9da45d88787cb2fd5bee81.[Accessed April 29, 2019].

[25] J. H. Chuah, H. Y. Khaw, F. C. Soon and C. Chow, “Detection of Gaussian Noise and Its Level using Deep Convolutional Neural Network”, Proc. of the 2017 IEEE Region 10 Conference (TENCON), Malaysia, November 5-8, 2017.

[26] M. Teichmann, M. Weber, M. Zöllner, R. Cipolla and R.Urtasun, "MultiNet: Real-time Joint Semantic Reasoning for Autonomous Driving", IEEE Intelligent Vehicles Symposium, IV 2018, Changshu, China, June 26-30, 2018, pp. 1013-1020.

[27] Y. Lyu, and X. Huang, “Road Segmentation Using CNN with GRU”, 22nd International Conference on Information Visualization, 2018.

[28] Z. Zhang, Q. Liu, Y. Wang. "Road extraction by deep residual U-net", IEEE Geosci. Remote Sens. Lett., vol. 15, no. 5, pp. 749-753, May 2018.

[29] J. G. Haran, J. Dillenburg, and P. Nelson, "Realtime Image Processing Algorithms for the Detection of Road and Environmental Conditions", Ninth International Conference on Applications of Advanced Technology in Transportation, AATT 2006, Chicago, Illinois, August 13-15, 2006, pp. 55-60.

[30] C. V. Dung and L. D. Anh, "Autonomous concrete crack detection using deep fully convolutional neural network", Automation in Construction, Volume 99, Pages 52-58, March 2019.

[31] J. Zhao, H. Wu, and L. Chen, “Road Surface State Recognition Based on SVM Optimization and Image Segmentation Processing,” Journal of Advanced Transportation, Vol 2017, pp. 1-21. 2017.

[32] Z. Wan-zhi, W. Zeng-cai, “Rural Road Detection of Color Image in Complicated Environment”, International Journal of Signal Processing, Image Processing and Pattern Recognition, Vol. 6, No. 6(2013), p.p. 161-168.

[33] M. Lin, Q. Chen, and S. Yan, “Network in network”, arXiv preprint arXiv:1312.4400, 2013.

[34] K. Simonyan and A. Zisserman, “Very deep convolutional networks for large-scale image recognition”, arXiv preprint arXiv:1409.1556, 2014.

[35] C. Szegedy, W. Liu, Y. Jia, P. Sermanet, S. Reed, D.Anguelov, D. Erhan, V. Vanhoucke, and A. Rabinovich, “Going deeper with convolutions”, In Proceedings of the IEEE Conference on Computer Vision and Pattern Recognition, pages 1–9, 2015.

[36] J. Dean, G. Corrado, R. Monga, K. Chen, M. Devin, M.Mao, A. Senior, P. Tucker, K. Yang, Q. V. Le, et al. “Large scale distributed deep networks”, In Advances in Neural Information Processing Systems, pages 1223–1231, 2012.

[37] J. Eriksson, L. Girod, B. Hull, R. Newton, S. Madden, and H. Balakrishnan, “The pothole patrol: using a mobile sensor network for road surface monitoring,” In Proceedings of the 6th international conference on Mobile systems, applications, and services (MobiSys'08), New York, USA, June 17 - 20, pp. 29-39.

[38] H. Zhao, J. Shi, X. Qi, X. Wang, J. Jia, “Pyramid Scene Parsing Network”, arXiv preprint arXiv:1612.01105v2[cs.CV] 27 Apr 2017.

[39] V. Badrinarayanan, A. Kendall, & R. Cipolla (2017), Segnet: A deep convolutional encoder-decoder architecture for image segmentation, IEEE transactions on pattern analysis and machine intelligence, 39(12), 2481-2495.

[40] M. Teichmann, M. Weber, M. Zoellner, R. Cipolla, & RUrtasun, (2018, June), Multinet: Real-time joint semantic reasoning for autonomous driving. In 2018 IEEE Intelligent Vehicles Symposium (IV) (pp. 1013-1020). IEEE.

[41] T. Pohlen, A. Hermans, M. Mathias, B. Leibe, “Full Resolution Residual Networks for Semantic Segmentation in Street Scenes”, arXiv:1611.08323v2 [cs.CV] 6 Dec 2016.

[42] Moran, Jeffrey, and Robert Desimone. "Selective attention gates visual processing in the extrastriate cortex." Science 229.4715 (1985): 782-784.

[42] Fei-Fei Li, Justin Johnson and Serena Yeung. CS231n. Class Lecture, Topic: “Convolutional Neural Networks for Visual Recognition.” Stanford University, Stanford, California 94305, Spring 2017.

[43] Beck, Joseph E., and Beverly Park Woolf. "High-level student modeling with machine learning." International Conference on Intelligent Tutoring Systems. Springer, Berlin, Heidelberg, 2000.

[44] Spanhol, Fabio Alexandre, et al. "Breast cancer histopathological image classification using convolutional neural networks." Neural Networks (IJCNN), 2016 International Joint Conference on. IEEE, 2016.

[45] LeCun, Yann, Koray Kavukcuoglu, and Clément Farabet. "Convolutional networks and applications in vision." Circuits and Systems (ISCAS), Proceedings of 2010 IEEE International Symposium on. IEEE, 2010.

[46] https://www.tensorflow.org/api\_docs/python/tf/keras/initializers/HeUniform

[47] Zou, Hui, and Trevor Hastie. "Regularization and variable selection via the elastic net." Journal of the Royal Statistical Society: Series B (Statistical Methodology) 67.2 (2005): 301-320.

[48] Srivastava, Nitish, et al. "Dropout: A simple way to prevent neural networks from overfitting." The Journal of Machine Learning Research 15.1 (2014): 1929-1958.

[49] Duchi, John, Elad Hazan, and Yoram Singer. "Adaptive subgradient methods for online learning and stochastic optimization." Journal of Machine Learning Research 12.Jul (2011): 2121-2159.

[50] Zeiler, Matthew D. "ADADELTA: an adaptive learning rate method." arXiv preprint arXiv:1212.5701 (2012).

[51] Hey, Anthony JG, and Anne E. Trefethen. "The data deluge: An e-science perspective." (2003): 809-824.

[52] Hecht-Nielsen, Robert. "Theory of the backpropagation neural network." Neural networks for perception. 1992. 65-93.

[53] Rumelhart, David E., Geoffrey E. Hinton, and Ronald J. Williams. "Learning representations by back-propagating errors." nature 323.6088 (1986): 533.

[54] LeCun, Yann, et al. "Backpropagation applied to handwritten zip code recognition." Neural computation 1.4 (1989): 541-551.

[55] Özgenel, Çağlar Fırat (2019), “Concrete Crack Images for Classification”, Mendeley Data, v2

[56] Lei Zhang , Fan Yang , Yimin Daniel Zhang, and Y. J. Z., Zhang, L., Yang, F., Zhang, Y. D., & Zhu, Y. J. (2016). Road Crack Detection Using Deep Convolutional Neural Network.

[57] Keras. Image data preprocessing (2021). https://keras.io/api/preprocessing/image/

[58]Vaibhav Khandelwal. The Architecture and Implementation of VGG-16 (2020). https://medium.com/towards-artificial-intelligence/the-architecture-and-implementation-of-vgg-16-b050e5a5920b

[59] Wikipedia. ImageNet (2021). <https://en.wikipedia.org/wiki/ImageNet>

[60] Wikipedia. Overfitting (2021). <https://en.wikipedia.org/wiki/Overfitting>

[61] Vitaly Bushaev. Adam — latest trends in deep learning optimization (2018). https://towardsdatascience.com/adam-latest-trends-in-deep-learning-optimization-6be9a291375c

[62] S Maitra, RK Ojha and [K Ghosh](https://scholar.google.com/citations?user=_ZvzkwIAAAAJ&hl=en&oi=sra). ‘Impact of Convolutional Neural Network Input Parameters on Classification Performance’ 2018 4th International, 2018.